|  |  |
| --- | --- |
| **Title:** | **DKS 3000 DKS 3000 –SELF-SUPPORTING DOUBLE SKIN METAL FACED INSULATING PANELS — FACTORY MADE PRODUCTS — SPECIFICATION** |
| **Document Type:** | PUBLIC REVIEW DRAFT  |
| **Dates:** | Circulation date | Closing date |
| 18th July 2024 | 19th September, 2024 |
| **Recipient** | **This form is to be filled, signed and returned to Kenya Bureau of Standards for the attention of Nkatha Betty (****nkathab@kebs.org****)** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Organization** | **Standard number** | **Clause** | **Paragraph/ Figure/Table** | **Type of comment (General/Technical /Editorial)** | **COMMENTS** | **Proposed Change** |
| EXAMPLEKEBS | KS 223 | **2.3**  | 1 | Technical | There is no mention of electrolyte density in relation to climatic differences.  | Include requirements for batteries intended for use in tropical and equatorial climates |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |